Pasewalk, May 27th, 2016

REMOS GXiS Takes Off for Maiden Flight

**On May 26th, 2016, the REMOS GXiS took off for its maiden flight after the ground tests were successfully completed and the required permissions were issued by the authorities.**

First we did some taxi tests with increasing speed until the nose wheel came up. At 11:20 UTC pilot and engineer Christian Majunke took off for the first flight from the runway in Pasewalk. In total he and Daniel Browne spent about one hour in the air. All values were in the green and the aircraft behaved as expected: Just great like every REMOS does. The full speed range from stall to high speed cruise was flown.

What will happen next? This first flight marks the kick-off for the flight tests required for the European LSA certification. For this, an excessive flight test campaign has to be accomplished. Christian Majunke: “We will fly the aircraft throughout its entire flight envelope up to the maximum load factors, take off and landing performance, noise tests, spinning, flutter and many more. Plenty of work – let’s go!”

Our goal is to certify the GXiS both as CS-LSA and ultralight aircraft in Europe. We’ll also offer the aircraft in the USA as an ASTM-compliant LSA. The GXiS is the first REMOS powered by the Rotax 912 iS Sport fuel injected engine. To make the start-up procedure as easy as possible, REMOS invented a system called SMARTstart – almost all checks are done automatically now. The REMOS GXiS also offers a state-of-the-art avionics suite.

**Images are free for publication with copyright note „REMOS AG“.**

Press contacts:

REMOS AG   
Franzfelde 31   
17309 Pasewalk  
Germany

Sales: Jürgen Rehländer  
juergen.rehlaender@remos.com  
Tel.: +49 170 3468616

Public Relations & Marketing: Patrick Holland-Moritz   
 patrick.holland-moritz@remos.com   
 Tel.: +49 151 46533333